## Vor Ort Notes

1. Plane Switch Portbelegung
2. Stelle alle Geraete auf dhcp um: 
	1. [x] switches
	2. [x] APs
	3. [x] Cloud-Key
	4. [x] Telefone
	5. [x] Drucker (drucker muss mehr angepasst werden: dns)
3. Dangerous: Setze VLANs auf designierte Ports um
4. Geraete runterfahren
5. Neue Firewall anschalten und hoffen, dass es klappt

## Notes
opnsense ui: root,  4H?bh,wXU85JrXs
opnsense ui: sbxadmin, %bghY!FH65Z
cloud key: user: sbxadmin, 'l0b-J3HbQ7Om0jbfeuah' 
Main switch: 60:22:32:ee:22:38
Subscription key: a119bcee-9ca0-438c-b2c9-69db51d186b8

## General
- [ ] hermann ablauf mitteilen
- [ ] Internetzugangsdaten beschaffen
- [x] pruefe WAN/Modem Anschluss - fritz macht pppoe als router; modem laut fritz vorhanden - entferne fritzbox

- [x] Change public DNS entries (gw.studio-stadt-region.de -> \<public-ip\> )
- [x] ports der unifi untersuchen
- [x] configure dhcp on all unifi devices
- [x] acme - challenge type - andere token con cf
- [x] unifi dashboard - define all vlan networks
- [x] add to opncentral
- [x] fotos machen
- [x] unifi cloud key mit cloud koppeln
- [ ] Switch und APs in IT-Glue hinterlegen
- [ ] physische Beschriftung anpassen


### deprecated
- [ ] ips/ids anschalten
- [ ] change ilo ip such that its in the mgmt net
- [ ] backup via ftp to nas if possible


## Kerio Features 

### Network

- WAN: 10.0.80.2 (FritzBox PPPoE)
- LAN: 192.168.80.1/24
- VPN: 172.16.80.1/24

### DNS and DHCP

- [x] domain name: ad.studio-stadt-region.de
- [x] query forwarding: `*.zvelo.com` -> `1.1.1.1,1.2.2.1`

## OPNsense

### Network

| Name       | Interface | VLAN tag | Network         | Note                    |
| ---------- | --------- | -------- | --------------- | ----------------------- |
| WAN        | WAN       | /        | 10.0.80.2/32    | FritzBox PPPoE          |
| MGMT       | LAN       | 1        | 192.168.50.1/24 |                         |
| SERVER     | LAN       | 80       | 192.168.80.1/24 |                         |
| CLIENT     | LAN       | 20       | 192.168.20.1/24 |                         |
| WLAN       | LAN       | 30       | 192.168.30.1/24 | USE CLIENT net for WLAN |
| WLAN_GUEST | LAN       | 40       | 192.168.40.1/24 |                         |
| OpenVPN    | VPN       |          | 172.16.80.1/24  |                         |

### Firewall

#### Aliase

- [x] filewave
- [x] mailstore
- [x] nas
- [x] sbxoffice
- [x] ad
- [x] printer (NEW IP: 192.168.20.10. OLD IP: 192.168.80.200)
- [x] phone (NEW IP: 192.168.20.28/29. OLD IP: 192.168.80.28/29)

#### Rules

##### WAN

- [ ] enable geo filter (iran, north korea, russia)
- [ ] Allow VPN entrypoint to WAN via VPN port

##### MGMT

- [ ] allow 'mgmt addr' to AD server via ldap
- [ ] allow 'mgmt net' to AD via dns

##### USER

- [ ] allow 'user net' to AD via dns
- [ ] allow 'user net' to nas via smb
- [ ] allow 'user net' to AD via ldap(s)
- [ ] allow 'user net' to 'server net' via https
- [ ] allow 'user net' to mailstore via its web port (Reverse Proxy in future)
- [ ] allow 'user net' to vwlizenz via (any?)
- [ ] allow 'user net' to filewaveserver via filewaveservice ports

##### VPN

- [ ] allow 'vpn net' to AD via dns
- [ ] Allow SMB for VPN Client network
- [ ] allow vpn net to server net

##### SERVER

- [ ] Allow filewave out 

#### DNAT

- [ ] Port 8462/tcp from WAN address to Mailstore IP NAT
- [ ] Port Group "Filewave" from WAN address to Filewave IP NAT

### Authentication Server

- [ ] AD coupling somehow - DNAT from sbxoffice to local AD via LDAP(s)

### VPN
- depends on: Authentication Server
- one user and one admin vpn server

- [ ] Setup OpenVPN. 
	- [ ] Self-Signed Certificate Chain: Root CA, Server Cert and Client Cert
	- [ ] setup openvpn server
	- [ ] setup client certs

### IPS/IDS

- [ ] setup and configure surricata - very heavy on resources.. need to be tested

### Content Filter

- [ ] Recreate - if possible - application, web and https filter

### Reverse Proxy (Web Server Protection)

- [ ] projektpro
- [ ] Andere?

### NTP 

- Server: `srvu-master.ad.studio-stadt-region.de`

## Archive

